> Six-Trak Reinitialzation Procedure
> This page details the reinitialzation procedure for the Six-Trak. Warning: Do not attempt any of these procedures if you don't understand what is being discussed. Proceed at your own risk. If your Six-Trak is counting 1 to 6 when you first turn it on or it is is locked-up, you might want to try this before thinking about replacing the battery or having the synth serviced.

> Reinitialzation

> > > 1. Center the PITCH wheel. Hold CONTROL RECORD and press PROGRAM SELECT #3.
> > > 2. Hold TRACK RECORD then CONTROL RECORD, and press SELECT #0.
> > > The CONTROL RECORD LED will go off. Turn off the TRACK RECORD LED by pressing TRACK RECORD.
> > > 3. Press ARP UP/DOWN twice.
> > > 4. Press ARP ASSIGN twice.
> > > 5. Press STACK A twice.
> > > 6. Press STACK B twice.
> > > 7. Press TRACK RECORD then press SEQ A, then press TRACK RECORD.
> > > 8. Press TRACK RECORD then press SEQ B, then press TRACK RECORD.
> > > 9. Hold CONTROL RECORD, then press SELECT 8. This will load the Basic Patch into the Six-Trak's RAM.
> > > 10. Hold CONTROL RECORD, then press 00. This will save the Basic Patch into voice number 00.
> > > 11. Turn off the Six-Trak, then turn it on. If you lucky the Six-Trak will start correctly. If the synth is still counting from 1 to 6 or still "jammed" either proceed with the follow steps, or have the unit serviced. Steps #12 through #15 will erase all voices and sequences. Back-up your voices and sequences!!!
> > > 12. Expose the circuit board and locate the battery.
> > > 13. Lift one end of the diode (IN4002/ D108) coming from the positive side of the battery.
> > > 14. Touch pin 24 of one of the 6116s (U112, 117 and 119) to ground.
> > > 15. Reconnect the diode (see step #13).
> > > 16. Carry out steps #1 through #10.

> Back to NoteIt's Main page
© 1997-2000 noteit@juno.com

This page hosted by Get your own Free Home Page